SPI-CONFIG(1)

NAME
spi-config - set or query SPI configuration.

SYNOPSIS
spi-config options...

DESCRIPTION

Set or query the configuration of a SPI port.

-d, --device=DEVICE
    use the given Linux spidev character device.

-q, --query
    print the current configuration.

-m, --mode=[0-3]
    set the spi mode (see SPI MODES below).

-l, --lsb={0,1}
    set LSB first (1) or MSB first (0).

-b, --bits=[7...]
    set the number of bits per word.

-s, --speed=FREQUENCY
    set clock frequency (in Hz).

-h, --help
    display the help screen and exit.

-v, --version
    display the version number and exit.

  SPI MODES

mode 0
    low iddle level, sample on leading edge.

mode 1
    low iddle level, sample on trailing edge.

mode 2
    high iddle level, sample on leading edge.

mode 3
    high iddle level, sample on trailing edge.

EXAMPLES

Get help:
    $ spi-config -h

Query current configuration:
    $ spi-config --device=/dev/spidev0.0 -q

Change clock frequency to 1 MHz:
    $ spi-config --device=/dev/spidev0.0 --speed=1000000

AUTHOR
Written by Christophe BLAESS <http://www.blaess.fr/christophe>.

REPORTING BUGS
Github home page: <https://github.com/cpb-/spi-tools.git>

COPYRIGHT
Copyright © 2014 Christophe Blaess.
Licensed under GPLv2 <http://gnu.org/licenses/gpl.html>.
This is free software: you are free to change and redistribute it.
There is NO WARRANTY, to the extent permitted by law.